<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="99.9" y2="44.35" width="0" layer="20"/>
<wire x1="99.9" y1="44.35" x2="-0.1" y2="44.35" width="0" layer="20"/>
<wire x1="-0.1" y1="44.35" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="transistor-pnp">
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-fet">
<packages>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="transistor">
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler">
<packages>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<packages>
<package name="C5B7.2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 7.2 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="con-ptr500">
<packages>
<package name="AK300/2">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="relay">
<packages>
<package name="F4052">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Finder</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q9" library="transistor-pnp" package="TO92" value="BC557"/>
<element name="Q7" library="transistor-fet" package="TO220" value="BUZ10"/>
<element name="Q8" library="transistor-fet" package="TO220" value="BUZ10"/>
<element name="D4" library="diode" package="DO35-7" value="1N4148DO35-7"/>
<element name="D5" library="diode" package="DO35-7" value="1N4148DO35-7"/>
<element name="R10" library="rcl" package="0207/2V" value="10K"/>
<element name="R11" library="rcl" package="0207/10" value="100K"/>
<element name="R13" library="rcl" package="0207/12" value="10K"/>
<element name="Q3" library="transistor" package="TO92" value="BC547"/>
<element name="R6" library="rcl" package="0207/12" value="2K2"/>
<element name="OK1" library="optocoupler" package="DIL06" value="CNY17">
<attribute name="OC_NEWARK" value="05M4044"/>
<attribute name="MPN" value="CNY17-1"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1045399"/>
</element>
<element name="R1" library="rcl" package="0207/5V" value="22K"/>
<element name="OK2" library="optocoupler" package="DIL06" value="CNY17">
<attribute name="OC_NEWARK" value="05M4044"/>
<attribute name="MPN" value="CNY17-1"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1045399"/>
</element>
<element name="Q10" library="transistor-pnp" package="TO92" value="BC557"/>
<element name="Q6" library="transistor-fet" package="TO220" value="BUZ10"/>
<element name="Q5" library="transistor-fet" package="TO220" value="BUZ10"/>
<element name="D7" library="diode" package="DO35-7" value="1N4148DO35-7"/>
<element name="D6" library="diode" package="DO35-7" value="1N4148DO35-7"/>
<element name="R12" library="rcl" package="0207/10" value="10K"/>
<element name="R9" library="rcl" package="0204V" value="10K"/>
<element name="R14" library="rcl" package="0207/12" value="100K"/>
<element name="Q4" library="transistor" package="TO92" value="BC547"/>
<element name="R5" library="rcl" package="0207/12" value="22K"/>
<element name="R2" library="rcl" package="0207/12" value="2K2"/>
<element name="IC1" library="linear" package="TO220H" value="7805T"/>
<element name="R15" library="rcl" package="0207/7" value="220"/>
<element name="LED1" library="led" package="LED3MM" value="red"/>
<element name="Q2" library="transistor" package="TO92" value="BC547"/>
<element name="Q1" library="transistor" package="TO92" value="BC547"/>
<element name="R3" library="rcl" package="0207/12" value="10K"/>
<element name="R4" library="rcl" package="0207/12" value="2K2"/>
<element name="D3" library="diode" package="DO41-10" value="1N4002"/>
<element name="D2" library="diode" package="DO41-10" value="1N4001"/>
<element name="D1" library="diode" package="DO41-10" value="1N4001"/>
<element name="C2" library="rcl" package="E5-10,5" value="1000uF"/>
<element name="C1" library="rcl" package="E5-10,5" value="100uF"/>
<element name="C3" library="rcl" package="E5-10,5" value="2,2uF"/>
<element name="R16" library="rcl" package="0207/10" value="10 Ohm"/>
<element name="C6" library="capacitor-wima" package="C5B7.2" value="100nF"/>
<element name="R17" library="rcl" package="0207/10" value="10k"/>
<element name="X1" library="con-ptr500" package="AK300/2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X2" library="con-ptr500" package="AK300/2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="FIN_40-52-9_12V_2XUM" library="relay" package="F4052" value="4052">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R7" library="rcl" package="0617/17" value="0R33 3 Watt"/>
<element name="R8" library="rcl" package="0617/17" value="0R33 3 Watt"/>
<element name="U$1" library="avr-7" package="DIL08" value="TINY138P3"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="D5" pad="C"/>
<contactref element="R13" pad="1"/>
<contactref element="Q8" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D4" pad="C"/>
<contactref element="Q7" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D4" pad="A"/>
<contactref element="Q9" pad="3"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="Q7" pad="3"/>
<contactref element="R10" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R13" pad="2"/>
<contactref element="Q8" pad="3"/>
<contactref element="FIN_40-52-9_12V_2XUM" pad="P2"/>
</signal>
<signal name="N$7">
<contactref element="R11" pad="2"/>
<contactref element="Q9" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="OK1" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R11" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="OK2" pad="5"/>
</signal>
<signal name="N$14">
<contactref element="Q10" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R14" pad="1"/>
<contactref element="OK2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="D6" pad="C"/>
<contactref element="Q5" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="D7" pad="C"/>
<contactref element="R12" pad="1"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R12" pad="2"/>
<contactref element="Q6" pad="3"/>
<contactref element="FIN_40-52-9_12V_2XUM" pad="P1"/>
</signal>
<signal name="N$22">
<contactref element="D7" pad="A"/>
<contactref element="D6" pad="A"/>
<contactref element="Q10" pad="3"/>
</signal>
<signal name="N$24">
<contactref element="R5" pad="1"/>
<contactref element="OK1" pad="5"/>
<contactref element="Q4" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$25">
<contactref element="R9" pad="1"/>
<contactref element="Q5" pad="3"/>
<contactref element="Q4" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="C3" pad="+"/>
<contactref element="R17" pad="2"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="N$26">
<contactref element="R15" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="R3" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R4" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="Q2" pad="3"/>
<contactref element="OK2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="2"/>
<contactref element="Q9" pad="1"/>
<contactref element="OK1" pad="1"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$33">
<contactref element="Q1" pad="3"/>
<contactref element="D3" pad="A"/>
<contactref element="FIN_40-52-9_12V_2XUM" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="D2" pad="C"/>
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="R2" pad="2"/>
<contactref element="Q10" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="FIN_40-52-9_12V_2XUM" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="D2" pad="A"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="R17" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="X1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="OK1" pad="4"/>
<contactref element="IC1" pad="2"/>
<contactref element="LED1" pad="K"/>
<contactref element="Q4" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="C6" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="X1" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="OK2" pad="4"/>
<contactref element="Q3" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="X2" pad="2"/>
<contactref element="FIN_40-52-9_12V_2XUM" pad="O1"/>
<contactref element="FIN_40-52-9_12V_2XUM" pad="S2"/>
</signal>
<signal name="N$34">
<contactref element="X2" pad="1"/>
<contactref element="FIN_40-52-9_12V_2XUM" pad="S1"/>
<contactref element="FIN_40-52-9_12V_2XUM" pad="O2"/>
</signal>
<signal name="N$5">
<contactref element="Q7" pad="2"/>
<contactref element="Q8" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="Q5" pad="2"/>
<contactref element="Q6" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="3"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="6"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
